## Creality CR-10 - 300\*300\*400mm Printing Size

|  |  |
| --- | --- |
| **Specifications** | |
| Printing size | 300\*300\*400mm |
| Printing type | FDM (Melting touch stack molding technology) |
| Body structure | Patent technology V-Slot aluminum bearing |
| Nozzle diameter | Default 0.4mm, one 0.3mm nozzle for free |
| Filament diameter | 1.75mm |
| Plug | Default EU plug (the CN warehouse will ship the adapter together) |
| Print speed | ≤200mm / s, normal printing speed: 100mm / s |
| Each accuracy | 0.05-0.4mm (adjustable) |
| Power supply | Input 110-220V switchable, output 12V |
| Actual power | 160-200W |
| Operating page | Chinese / English |
| Printing accuracy | ±0.1mm |
| Environmental requirement | 10-30°C, humidity 20-50% |

|  |  |
| --- | --- |
| **Parameter** | |
| Materials | PLA, ABS, TPU, Copper, Wood, Carbon Fiber, Gradient Color etc. |
| Software supporting | PROE, Solid-works, UG, 3d Max, Rhino 3D design software, etc. |
| Format | STL, OBJ, G-Code, JPG |
| Printing method | SD card(off-line), contact to the PC(on-line) |
| Operating system | Linux, Windows, OSX |
| Operating software | CURA, Repetier-Host, simplify 3D |
| Machine size | 490\*600\*615 mm |
| Package size | 540\*640\*310 mm |
| Machine net weight | 10.3kg |
| Package weight | 14kg |